**I2C Relay Board**

A picture containing text, electronics, circuit

Description automatically generated

GPIO Driven Relay Control connector

I2C Addressing jumpers

I2C Relay Control connector

![A picture containing text, electronics, circuit

Description automatically generated]()

I2C connector, can be used to piggyback multiple boards

![A picture containing text, electronics, circuit

Description automatically generated]()

I2C Addressing jumpers

Left hand pads are ground

Right hand pads are 5VDC

Middle pads are address pins

Base address is 0x20.